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Membership for 2024
Full Member - $125.00 
Associate - $75.00

$50.00 1-Day temporary member (Temporary members do not receive points)
           Bylaws Of

SOUTHERN MISSOURI TRUCK AND TRACTOR PULLERS ASSOCIATION

Section 1: Name

The name of this not-for-profit organization is: Southern Missouri Truck and Tractor Pulling Association.

Section 2: Purpose

The organization is organized exclusively for charitable, religious, educational, and scientific purposes under section 501 (c) (3) of the internal Revenue Code, or corresponding section of any future federal tax code. These include:

A. To promote, develop, supervise, and voluntarily assist in all lawful ways the interest of members who will participate in truck and tractor pulling contests, preparation for contests and other related activities hereafter organized. To help and voluntarily assist members in developing qualities of citizenship and sportsmanship.

B. To promote truck and tractor pulling contests, to acquire by lease, purchase, or otherwise, and to own, hold and sell such real estate and personal property as may be necessary or convenient for the construction, maintaining, and operations of truck and tractor pulling contests for the use of its members, guest, and public; and to provide means and facilities for social friendship for its members and their guests, and to acquire by purchase, lease, or otherwise of a clubhouse, club rooms, and other equipment and to buy sell and acquire all necessary paraphernalia, goods, and merchandise, and to sell the same to its members, guest, and the public;  and to do all things necessary and incidental thereto.

C. To promote, foster, and encourage interest in truck and tractor pulling and other related activities; to establish and enforce rules of truck and tractor pulling competition sponsored by the corporation; to provide places for holding meetings; to rent, lease, acquire, and/or own such real and personal property as may be necessary; and to do all other legal powers permitted a Nonprofit Corporation.

Section 3: Location, Corporate Seal and Fiscal Year

3.1 Location -The principal office of the corporation shall be the address of the president unless otherwise specified by action of the board of directors. The registered office of the corporation may be, but need not be, identical with the principal office of the corporation, and the address of either office may be changed from time to time by the board of directors. The corporation also may have offices at such other places both within and without the State of Missouri as the board of directors may from time to time determine. Springfield, Missouri is the central hub of the Southern Missouri Truck and Tractor Pullers Association.

3.2 Corporate Seal-The directors may adopt and alter the seal of the corporation.

3.3 Fiscal Year-The fiscal year of the corporation shall, unless otherwise decided by the directors, end on the31st day of December of each year.

Section 4: Members

4.1 Qualification- of members. A member shall have full voting privileges. Individuals who desire to participate in the sport of pulling who have qualifications shall be eligible for membership in the corporation upon payment of the requisite membership dues.

4.2 Dues-The directors shall propose the dues necessary to become a member of the corporation. Each year at their annual meeting, the directors shall propose the amount of membership due to be determined by a majority of the votes of the members at the meeting. The membership is not refundable at the meeting or throughout the season.

4.3 Resignation- A member may resign from the corporation by delivering a written resignation to the president, treasurer, or secretary of the corporation at its principal office. Such resignation shall be effective upon receipt (unless specified to be effective at some other time), and acceptance thereof shall not be necessary to make it effective unless it states.

4.4 General Meetings-The annual meetings may be held at such places, either within or without the State of Missouri, as the board of directors shall determine. At the annual meeting, the previous year's business shall be reviewed, goals set for the coming year, the board's recommendations for the general contest rules including specific class rules and bylaws shall be reviewed and modified as determined necessary by majority vote of the members. Also, the election for eligible board positions shall take place at this time. The new board shall be installed at the January board meeting following the annual meeting.

4.4.1 Special Meetings-Special meetings of the members may be held at any time and at any place, either within or without the State of Missouri, as designated in the notice of the special meeting. Special meetings of the members may be called by the president or by the directors and shall be called by the secretary upon written application of members having one-tenth of the votes entitled to be cast at such meeting, or by100 members if the number of members entitled to vote at such meeting shall exceed 1,000.

4.5 Call and Notice - Written notice stating the place, day and hour of the meeting of members and, in the case of a special meeting, the purposes for which the meeting is called, shall be delivered not less than five, nor more than 40 days, before the date of the meeting, personally by mail or by email. If the notice is mailed, such notice shall be deemed to be delivered when deposited in the United States mail addressed to the member at his address as it appears on the records of the corporation, with postage prepaid.

4.6 Quorum -At any meeting of the members, one-third (1/3) of the members then in good standing shall constitute a quorum.

4.7 Action by Vote- Each member shall have one vote. When a quorum is present at any meeting, a simple majority of the votes properly cast by the members present in person shall decide any question, including election to any office, unless otherwise provided by law, the articles of incorporation, or these bylaws. To be eligible to vote on class rules you must have participated in 50% of the pulls of the previous year or be actively involved in the organization, at the board's discretion.

4.8 Order-All meetings shall be held in an orderly fashion, any member who is not acting in an orderly fashion shall be removed and suspended from association events for up to (30) days at the decision of the board after notice to the disorderly member an opportunity to be heard.

Section 5: Board of Directors

5.1 Number and Election - The number of directors shall be seventeen consisting of the President, Vice President, Secretary, Treasurer and Thirteen members at large elected at the annual meeting and installed at the December meeting.

5.2 Tenure-Each director shall hold office until the January board meeting after the election and until his or her successor is elected and qualified, or until he or she dies, resigns, is removed or becomes disqualified. Terms consist of Three years, terms as to not have all positions elected at the same time. 

5.3 Powers-The affairs of the corporation shall be managed by the directors who shall have and exercise all the powers of the corporation, except those powers reserved to the members by law, the articles of incorporation, or these bylaws.

5.4 Committees - The directors may elect or appoint one or more committees, which shall consist of two or more directors and can have members who are not directors. The directors may delegate to any such committee or committees any or all their powers. Unless the directors otherwise designate, committees shall conduct their affairs in the same manner as is provided by these bylaws for the directors. The members of any committee shall remain in office at the pleasure of the directors.

5.5 Suspension or Removal - A director may be suspended with or without cause by vote of simple majority of the board of directors. A director may be removed with cause only after reasonable notice and opportunity to be heard by the members.

5.6 Resignation-A director may resign by delivering his or her written resignation to the president, treasurer or secretary of the corporation, to a meeting of the members or directors or to the corporation at its principal office. Such resignation shall be effective upon receipt (unless specified to be effective at some other time) and acceptance thereof shall not be necessary to make it effective unless it states so much. 

5.7 Vacancies - Any vacancy in the board of directors may be filled by the directors provided, however, that the members also have the power to fill vacancies in the board of directors. Each successor shall office for the unexpired term or until he dies, resigns, is removed or becomes disqualified. The directors shall have and may exercise all their powers notwithstanding the existence of one or more vacancies in their number.

5.8 Regular meetings of the directors may be held at such places and at such times as the directors may determine.

5.9 A Special Meetings-Special meetings of the directors may be held at any time and at anyplace were called by the president or by two or more directors.

            5.9 B. SMTTPA General Board Members 
The SMTTPA general Board will consist of 14 members. They will help with making decisions along with the Executive Officers of the Board. The members of the association will vote every three years for new members to fill these positions. 
ALL BOARD MEMBERS MUST PARTICIPATE AT LEAST 50% OF THE PULLS AND 50% OF THE BOARD MEETINGS. IF THE BOARD MEMBER IS A FULL OR ASSOCIATE MEMBER OF A TRACTOR OR A TRUCK, THEY MUST PULL THAT VEHICLE AT LEAST 50% OF THE SANCTIONED PULLS TO BE ELIGIBLE TO CONTINUE AS A BOARD MEMBER. IF A BOARD MEMBER OWNS A PULLING TRUCK OR TRACTOR, THEY MUST MEMBER THAT VEHICLE WITH SMTTPA, THEY ARE ALSO ELIGBLE TO MEMBER SAID VEHICLE WITH ANOTHER ASSOCIATION AS LONG AS THEY ARE A MEMBER OF SMTTPA (SPECIAL CONSIDERATIONS WILL BE DETERMINED BY THE EXECUTIVE BOARD)
5.10 Call and Notice

A. Regular Meetings-No call or notice shall be required for regular meetings of directors unless otherwise required by law, the articles of incorporation or these bylaws.

B. Special Meetings-Notice of the time and place of special meetings of the directors shall be delivered to each director not less than five or more than 40 days before the date of the meeting, either personally or by mail. If the notice is mailed, such notice shall be deemed to be delivered when it is deposited in the United States mail addressed to the director, with postage prepaid. Such notice need not specify the purposes of a meeting, unless otherwise required by law, the articles of incorporation or these bylaws.

5.11 Quorum -At any meeting of the directors, 2/3 of the directors then in office shall constitute a quorum. Any meeting may be adjourned by majority of the votes cast upon the question, whether a quorum is present, and the meeting may be held as adjourned without further notice.

5.12 Action by Vote -When a quorum is present at any meeting, 2/3 of the directors’ present and vote shall decide any question, unless otherwise provided by law, the articles of incorporation or these bylaws. All officers and board members have one vote each.

5.13 Action by Writing - Any action required or permitted to be taken at any meeting of the directors may be taken without a meeting if all the director’s consent to the action in writing and the written consents are filed with the records of the meetings of the directors. Such consents shall be treated for all purposes as a vote at a meeting.

Section 6: Offices

6.1 Number and Qualification - The offices of the corporation shall be a president, vice president, secretary, treasurer, and such other officers, if any, as the directors may determine. The Corporation may also have such agents, if any, as the directors may appoint. If required by the directors, any officer shall give the corporation a bond for the faithful performance to his/her duties in such amount and with such surety or certainties as shall be satisfactory to the directors.

6.2 Election -After the first set of officers are elected, the officers shall be elected at the end of 3-year term by the members at the annual meeting. Other officers, if any, may be elected by the directors at any time or terms not exceeding three years.

6.3 Tenure- The offices shall each hold office until the successor is chosen qualified, or until he or she sooner dies, resigns, is removed or becomes disqualified. President, Vice President, Treasurer and Secretary are elected to three-year terms.

6.4 President- the president shall be the chief executive officer of the corporation and subject to the control of the directors, shall have general charge and supervision of the affairs of the corporation. The president shall preside at all meetings of the members and at all meetings of the directors, except as the members of directors otherwise determine.

6.5 Vice President-The vice president shall have such duties and powers, as the directors shall determine. The vice president shall have and may exercise all the powers and duties of the president during the absence of the president or in the event of his inability to act.

6.6 Treasurer-The treasurer shall be the chief financial officer and the chief accounting officer of the corporation. The treasurer shall oversee its financial affairs, funds, securities and valuable papers and shall keep full and accurate records thereof. The treasurer shall have such other duties and powers as designated by the board of directors or the president. The treasurer shall also oversee its books of account and accounting records, and of its accounting procedures. The treasurer shall be empowered to execute corporation checks along the President, Vice-President, and Secretary, which shall require two signatures from different families.

6.7 Secretary-The secretary shall record and maintain records of all proceedings of the members and directors in a book or series of books kept for that purpose, which shall be open at all reasonable times to be inspected by any member. Such books or books shall also contain records of all meetings of incorporators and the original or attested copies, of the articles of incorporation and bylaws and names of all members and directors and the address or each.

6.8 Suspension or Removal - A director may be suspended with or without cause by vote of simple majority of the board of directors. A director may be removed with cause only after reasonable notice and opportunity to be heard by the members. The President can suspend any director, until the board is able to meet and discuss actions. 

6.9 Resignation - A director may resign by delivering his or her written resignation to the president, treasurer or secretary of the corporation, to a meeting of the members or directors or to the corporation at its principal office. Such resignation shall be effective upon receipt (unless specified to be effective at some other time) and acceptance thereof shall not be necessary to make it effective unless it states so much.

6.10 Vacancies-If the office of any officer becomes vacant, the directors may elect a successor. Each successor shall hold office for the unexpired term, and in case of the president, vice president, treasurer and secretary until a successor is elected a qualified, or in each case until her or she sooner dies, resigns, is removed or becomes disqualified.

Section 7: Execution of Papers

Except as the directors may authorize the execution thereof in some other manner, all deeds, leases, transfers, contracts, bonds, notes, and other obligation made accepted or endorsed by the corporation shall be approved by the board of directors and signed by the president, the vice president, and one other board member. 

Any reasonable instrument purporting to affect an interest in real estate, executed in the name of the corporation by two of its officers, of whom one is the president or a vice president and the other is the treasurer or secretary, shall be binding on the corporation in favor of a purchaser or the person relying in good faith on such instrument notwithstanding and inconsistent provisions of the articles of incorporation, bylaws, resolutions or votes of the corporation.

Section 8: Personal Liability

The members, directors and officers of the corporation shall not be personally liable for any debt, liability or obligation of the corporation. All persons, corporations or other entities extending credit to, contracting with, or having any claim against the corporation may look only to the funds and property if the corporation for the payment of any such contract or claim, or for the payment of any debt damages, judgment or decree, or of any money that may otherwise become due or payable to them from the corporation.
Written on This Day on the 13th of March 2026.

President: Gary Verch 






Secretary: Jessica Breheim
                           General Contest Rules
1)  You must be an S.M.T.T.P.A. member to pull in all sanctioned classes for points.  Entry Fees for members are $30.00.  For 1-day temporary membership (1 time hook) $50.00. (NO REFUNDS) All temporary members must conform to the rules and by-laws of the association. If your vehicle is found to be illegal it will be an exhibition hook only. (NO POINTS/NO MONEY) The vehicle must be a member to hook to   the sled, in sanctioned classes, at any of our pulls, due to insurance reasons.
Membership Dues: Full Members 125.00   Associate Members 75.00                         1 Day Temporary Membership $50.00
1) ALL Pullers need to be signed in 45 minutes be the start of the pull or you will be subject to pay additional $20.00 LATE FEE (NO EXCEPTIONS) Members: $50.00 Temporary Members: $70.00 You may enter when you arrive if class has already started but your placement in in the lineup will be by a member of the Board There will be no complaints to the registration table or scales. You must see an Official Board member for all complaints. If you fail to do so you will be Disqualified for that night (NO POINTS, NO MONEY, NO REFUND)
2)
A number must be drawn for every puller to know what pulling position they will be pulling in.   Class Line-up - No changing classes around for people to get there and pull. You can call, but a number will be drawn for you by the person at table and you are responsible for getting the hook fee to table before you pull along with signing the release before you hook to the sled.  If you are not there in time to pull, you forfeit your pull but still must pay the hook fee if you are on the roster.
3)     All pulling vehicles must have full membership. If a vehicle has more than one driver, the other driver can sign up as an associate member. If you have two or more Trucks/Tractors you must have full membership of each vehicle. Associate members can only drive on the membership that they are signed up for. 
4) A sanctioned pull must use a dirt track no less than 300 feet in length, and not less than 30 feet in width. The track must be maintained and supplied with the proper equipment during the pull.  Trucks and Tractors to have a floating gate except in circumstances where a floating gate is not possible, i.e., saddle clubs, rodeo arenas, ditches or other obstructions at the end of the track, etc.....
5) It is the puller’s responsibility to know who pulls in front of them, get in line, weigh in and get up to the sled when it is their turn to pull. We will only wait one (1) minute, Failure to be ready to hook in one minute, unless of mechanical trouble, we will go on to the next puller. 
6)
It will be the pullers’ responsibility to notify the track officials of troubles, or they will be disqualified.
7)
Vehicles traveling the farthest distance before being stopped will be declared the winner of their class.  If more than one vehicle goes through the course, more weight will be added; those vehicles will pull again, if mechanically possible.
8)
All pulls will be measured with a laser or a monitor on the sled.
9)
The sled operator and/or the president will make the decision on reweighting the sled.  
10)
If the puller tries to stop before 100' - a repull will be allowed if:
Front of Sled Stops before the 100’ Mark.
i.e., Laser/Sled Monitor Reads less than 100.00.’

The Sled Operator and the 100-foot flagger will be the final judges.
11)    First puller has the option to repull in 6th or last; if the sled is reweighted you have the option to back up and hook right then or puller can drop to the 6th or last position.
12)   A pull is not ended if the vehicle is hooked to the sled or ruled so by track official.   Pulls are ended by the following:
Forward motion stops. (Excessive digging will not be allowed)        
Disqualification:
The driver does not remain seated with seat belt on.
Vehicle gets out of bounds, including the 100’ starting area, not the sled.
Starting under the red flag.
All weights must be securely fastened to the pulling vehicle.  If the weight used for ballast falls off and touches the ground, it is an automatic disqualification unless you are the first puller of your class.
13)
All pulls must start with a tight hitch, no jerking allowed.  Contestants will be allowed two consecutive attempts and 100 feet to start the sled.
14) 
 Cone must be placed to spot the sled before the sled comes back from previous hook.  Each contestant has the privilege of and the responsibility for spotting the sled for each of their attempts.  The sled operator must be notified of where the contestant wishes sled placed when previous vehicle unhooks from sled.  Once the sled is back at the starting gate it will not be moved for a puller. The sled driver will try to get it to the spot you want but will not spend much time moving the sled around just to satisfy you.
15)
A marker will be used to mark out of bounds with inside of marker to be the
            boundary.

16)
Each vehicle may enter only one (1) class; the open classes are not included. 
17)
All protests must be made before the prize money is handed out that night of the pull.  The protest fee is $500.00 If the protested vehicle is found to be illegal, they will lose money for that pull, and the vehicle is kicked out a year and one day. The protester will be returned his protest fee.  If the protested vehicle is found to be legal, the protested vehicle keeps the protest fee and all prize money, if any is involved.  Any vehicle that is found illegal in cubic inches the vehicle and owner will be suspended for one year and one day with loss of points for the entire year, even if the vehicle has been sold to someone else. A tech check does not constitute a protest.
18)
UNSPORTMANSHIP-Conduct which exists of violence and arguing. This will not be tolerated and will be dealt with by the executive and truck/tractor boards (This includes your crew members.) Suspensions up to and including one year and a day. 
19)
No drinking alcoholic beverages by any driver until after they have competed, or your vehicle does not go down the track, and you will not receive any points for the night. (THIS WILL BE STRICKLY ENFORCED)
20)
All pullers must drive their vehicle onto the track and back it to the sled.
21)
No vehicle is to be left running and unattended after it has crossed the scales.
22)      No adjustments to pulling vehicle one you cross the scales (except 2 Wheel   Drives
 23)
At the board’s discretion, they can check your truck/tractor at any time they see fit. If you refuse for any reason, it will result for you to be kicked out for a year and a day.
24)
No compressed canisters of any kind allowed in any of the classes (NOS, oxygen, propane, etc.)
25)      RULE SUBMISSIONS:   Rule submissions must be submitted in writing to a member of the executive board before the end of the last pulling event for the season. The board has the discretionary right to deny or approve any rule submission that is submitted.  
26)
No Profanity or obscenity allowed on any vehicle.
27)      No traction control (including grid system or timing control on any truck).
28)      No coaching from the sidelines (including electronic communication from 
           anyone on the sidelines to the driver).
29)      You must drive your own vehicle onto the track (including backing to the sled).
            Tractor pullers may need help backing to the sled to be hooked up. 
                                                                   Points System: 

For a class of vehicles to be considered a points class at the end of the year at least three vehicles had to have pulled for points in at least 50% of the total pulls of the year.

1 point show & 5 points hook.
1st place ……10 points


6th place……5 points
                        2nd place …... 9 points


7th place……4 points
3rd place …… 8 points


8th place …...3 points
4th place …… 7 points


9th place …...2 points
5th place……  6 points
                        10th place…..1 point 
  In the event of a rain out (if the class has started) Each participant will get 6 points each. 
 Points will be awarded by what position you receive, regardless of 
Disqualification draws only points (5)
(Loss of weight, out of bounds, etc.)
Drawbar Heights
4 Wheel Drive – 26 inches
2 Wheel Drive – 30 inches
2 Wheel Drive over 540 CI - 28 inches 
All Tractors – 20 inches
Length from Center of Rear Axles to Hitching Point
4 Wheel Drive – 36% of wheelbase
2 Wheel Drive – 18” minimum All Tractors – 18” minimum
                                                     General Truck Rules
All drivers are required to wear fire jackets, pants, leather shoes, or racing shoes, full-faced helmet, seatbelt or harness, and neck braces. Helmets must be DOT or SNELL rated.  Gloves are optional but strongly encouraged.
1) TIRES: MAY BE BUFFED.  MUST BE DONE AT BOARDS APPROVED LOCATION.  ANY OTHER BUFFING/GRINDING WILL BE CAUSE FOR SUSPENSION FOR 1 YEAR AND 1 DAY AT BOARDS DISCRESTION.

2)
Open hood for inspection.
3)
No fuel tanks. No fuel pressure gauges or fuel lines inside of the cabs.
4)
If the battery is inside the cab, it must be safely enclosed and securely fastened down.
5)
No radiators or water hoses allowed inside the cab.
6)        A 2 ½-pound fire extinguisher must be mounted in the cab with easy reach of 
           driver. 
7)        Seat belts are required and must be worn when vehicle is pulling, or puller will be
            Disqualified.   
8)
Pumping: A class member may pump a member of class for $500.00 (Pump fee goes to the Association). Results will be given to members requesting pump. No disqualification. Vehicles will continue to compete unless found illegal by teardown. The top 5 vehicles can be pumped at board's discretion.
9)
Drawbar must be equipped with a steel hitching device not less than 1” by 1” square (1” round stock) and with a T round hole min. of 3 x 3 3 3/4 round hole.

10)
Hitch point to rear axle center, line must be a minimum of 36% of wheelbase and a max of 26” in height.
11)
Hitch points must be secure to vehicle frame and rigid in all directions.   No cables or chains allowed in hitch mounting.  Movement of the hitch in any direction will not be allowed. CLASS RULES APPLY.
12)
No cam types of rear ends.
13)
All drive line U joints are to be enclosed in 360 degrees shield 1/16-inch-thick steel or 1/8-inch aluminum. Shield should be rigid and close enough to joint to restrain any broken parts.  Joints should not be seen from side, top or bottom.
14)
Each drive shaft must have a minimum of (2) two loops. If a vehicle has a shaft between transmission and transfer case no longer than 24 inches, one (1) loop, properly centered, will suffice.  Two-piece shafts must have four (4) loops.
15)
Loop location to be no less than six (6) inches and no more than twelve (12) inches on solid end of shaft and one (1) inch past stub on end with slip joint, or three (3) loops evenly spaced so that if slip joint breaks, shaft cannot drop.
16)
Loop material shall be of steel no less than ¾ inch wide ¼ inch thick, if aluminum, minimum 3/8 inch thick.
17)
If the original vehicle has side doors they need to be on and closed.  Driver’s door must be operational from inside and outside. Bumpers, tailgates, van rear doors are optional.  Truck bodies may be fiberglass-complete body or body components.
18)
All weights must be securely attached to the vehicle. Loose ballast (sandbags, rocks, unattached metal, etc.) Not allowed.

19)
No dual wheels, chains, or studded tires allowed. All tires must have rubber or rubber compound contact between tire and pulling surface.
20)
Front and back glass or plexiglass required.  Tinted or shaded windows hindering the driver’s vision front or back will not be allowed.
21)
Any truck with engine-driven fan blade is required to have fan shroud and should be no more than one (1) inch from radiator core and ½ inch past rear blade.
22)
All pulling trucks must be required to have a steel billet flywheel.  The flywheel must be made of steel with the following mechanical properties: Tensile strength of 60,000 PSI and yield strength of 40,000 PSI. Any aluminum or magnesium fly specs will be acceptable. 
23)
All Trucks classes must be equipped with steel bell housing (SFI approved) plus a block saver plate.  A safety blanket is required for automatic transmissions.  
24)
Any type of metal shield to cover all axle bolts is mandatory and must be securely held in place.
25)
All pullers under the age of 18 need to be certified by the board for approval. Certification will be on playday/before or after a sanctioned pull.  A parental consent form must be signed. NO EXCEPTIONS
26)       NO KILL SWITCH/NO PULL   A working kill switch and back-up light located in the rear on the bed in all classes. Kill Switch must have a zip tie.  In the event your kill switch is pulled, and if the zip tie is broken, you can re hook, if the tie is NOT broken, you cannot re hook.
27)
Air-shocks, Airbags are NOT allowed.
28)
No flatbed, Diesel’s engines and no aluminum beds.
29)
Must have working Front Brakes or working Drive line Brake at transfer case.
30)
The back of engine blocks no closer than 14” (plus or minus .250”) to center line of front axle.
31)
Firewall must be original or of equal material strength. No open holes.
32)
Must run pump gas or racing fuel.  No alcohol or nitrous oxide.
33)       Natural Aspirated Engine Only.  
34)
No aftermarket fuel injection systems.
35) 
Must maintain stock Wheelbase max – 133”
36)
1 Ton front/ end max. Can run any rear end.  
37)
Must run SFI approved harmonic balancer or must have shield.
38)
No barred tires.
39)
All Automatic Transmission Equipped Vehicles must have neutral/park safety switch!
40)       All Trucks must have an OEM appearing frame. 
Truck Classes
Hot Stock Class
General Trucks Rules Apply
1) Single carburetor, limited to a 4150-style flange.
2)
468 Cubic inch Limit
3)
6200 LB Class
4)
No Visible Weights
5) Factory OEM cast iron intake, and factory aluminum intake for year of vehicle or factory installed fuel injection with factory aluminum intake.  No added material.  No adapter plate may have 1” spacer plate with 2 paper thin gaskets.
6) Factory Production Cast Iron OEM Heads – No Hemi Heads – No Aluminum Heads.  The head must have factory Casting #’s on them in factory location.
7) No blocked suspension, no traction bars, one vertical bolt in springs and may have 4 clamps per side.
8)  OEM Transfer case and axles:1-ton max truck rear end, no other style rear ends allowed. 
9) All shackles must be in a stock location and fully functional, no blocks, no welded springs.  (9) Nine total factory springs, Limit of 2 rear shocks in factory position.  Shocks cannot be solid or welded.
10) Hitch point will not be closer to centerline of rear axle that 36% of wheelbase. 36% of the maximum allowable wheelbase (133”) is 47.88” See Picture below
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11)   Complete body less tailgate.  No fiberglass bodies must be stock appearing, front bumper in stock location, can have 6” air dam below front bumper. No cut-out beds.  Full interior in cab including seat, or racing seat, dash, door panels and factory glass.
12)
No straight pipes or headers.  Exhausts must run through mufflers and must exit one (1) foot rear of cab and turn down.  Cast Iron Exhaust Only
13)
Engine must be able to pull 16” of manifold vacuum or more, at 800 rpm (No vacuum pumps).  RPM’s to be checked with a digital tach. Must make vacuum hose easily accessible and mount to driver’s side inside fender well. Vacuum hoses must be no larger than 1/8 of an inch in diameter and no longer than 6 ft. Must be accessible on the driver’s side fender well.
14)
Street legal DOT tires (REFER TO RULE 1 GENERAL TRUCK RULES) and no larger than 33” tall and 12.5” wide or 305R tire size. Front tires cannot track past the center of rear tires or vice versa.
15)
No brush or grill guard

. 

16)      Can run headers with flat tappet cams. Must pull 14” of vacuum at 1000 RPM’S.
17)      Motor mounts in stock position for make and model of the truck.
18)      Any Rules agreed on will be enforced. If rules are not followed and truck if found to be illegal. It will not be allowed to pull for points or money that night. No Exception.
Small Block Super Stock Truck Class
All General Truck Rules Apply
Pro Street Rules for Chassis Rules
1) 430 Cubic Inch Limit with 1% Tolerance
2) All blocks must be cast iron with standard bore spacing and standard deck height. 
3) No LS or late model-style engines with overhead cams allowed. After-market blocks are allowed but no aluminum blocks are permitted.
4) Blocks Allowed: 
 
Chevy: Small block including the small 400.

Dodge: 318/360 Small block
                  Ford: Windsor 302/351, Cleveland 351 & 400M 
 No FE Style blocks allowed. 
5) Heads: Any OEM or aftermarket heads made of cast iron or aluminum that are made from this make of blocks mentions in rule 4.
6) Any intake manifold that will fit these heads are allowed, including spacers you must use to mount the Cleveland intake to the Cleveland style heads on the 400M Ford block.
7) Any single carb is allowed but No fuel injection is permitted.
8) Any ignition system, mad or electronic box MSD, etc., or whatever brand you choose is permitted. 
9) This class will run PRO STREET GENERAL RULES for the Chassis and the Engine rules for the Small Block Super Stock as listed Above. 
10) Safety Equipment must be in place just as it is in the Pro Street Truck Rules.
11) ALCOHOL ALLOWED: Must wear a complete fire suit with alcohol, (Jacket, Pants, Gloves, Boots, Mask and a Full-Face Helmet & Sock). Helmet must be DOT or SNELL rated,
6200 Super Street Truck Class
All General Truck Rules Apply
1) The cubic inch limit is 468 Displacement 6200 lbs.
2) OEM iron cylinder heads, NO Hemi Heads
3) Back of engine block may be no closer than 14 inches, plus or minus ¼ inch, behind center line of front axle. 
4) Single Carburetor, limited to a 4150-style flange.  A 4150 base 4-barrel carburetor max.
5) No Fuel injection systems.
6) No dry sump oil systems are allowed.
7) No rear shocks allowed.
8) Factory OEM cast iron intake only, must have factory casting numbers, can use aluminum spacer to adapt the intake to tall deck blocks.  Can run aluminum spacers to adapt oval port intake to rectangle port factory cast iron head (not to exceed ½ inch thick adapter) 2-inch maximum spacer/adapter from carburetor to intake, plus 2 ¼ inch gaskets.
9) Can have open headers but must aim to the rear of the cab.
10) No blocked rear suspensions or traction bars. No chains, cables, or devices on front other than OEM.  One vertical bolt in springs on rear springs is allowed.  No blocks on rear suspension or traction bar.  Chains allowed on rear. 
11) Shackles or spring hangers must be in place and functional. No blocks on frame or shackles to limit suspension system travel. No welding of springs.  Can clamp springs, Clamps cannot be longer than 3 inches, 4 clamps per side. 
12) You can run a bumper or a draw bar style hitch.  If pulling from rear bumper, the bumper must be mounted to rear of stock frames.  Can have bracing from center of bumper to frame rail but can extend no further than 24 inches forward from the end of the frame. Pulling hitch must be mounted to the bumper.  Can pull from a twisted clevis or similar device, (horizontal L hole) Hitch must be no more than 26 inches in height and at least 36% of the wheelbase from the center of rear axle. 36% of the maximum allowable wheelbase (133 inches) is 47.88. Hitch bracket shall extend not more than 2 inches above the frame rail at attachment point. Hitch brackets must be constructed of 2” x 2” x ¼ metal. The forward edge of hitch brackets shall not extend no further than 24 inches forward of hitch point.  See picture:
13)  No visible weights beyond factory bumper in factory position.  Weights may hang 6 inches below bumper and be covered by a 6-inch air dam.  Bottom of weights are a minimum of 8 inches above ground.
14)  No fiberglass body.  Body must be stock appearing; front bumper must be in stock location.  Can have 6-inch air dam below from bumper.  No cut-out beds.
15) Trucks must have complete body less tailgate. 
16) Front tires cannot track past the center of rear tires, or vice versa.
17) OEM transfer case and 1 ton axels.
18) Tire size is limited to DOT 33 x 12.50 or 305/70
19) Small block motors will be able to run aluminum dual plant intakes, no air gap style, and no external modifications.  The cubic inch limit on small block motors will be 383.  They can only run OEM cast iron heads and an OEM cast iron block, no aluminum heads or blocks. 
20) Any super street truck and up with engine driven fan blade is required to have metal fan shroud and shall be no more than one (1) inch from radiator core and ½ inch past rear blade.
21) All trucks are limited to a maximum 133-inch wheelbase. 
22) Any rules agreed on will be enforced. If rules are not followed and truck is found illegal, IT WILLNOT BE ALLOWED to pull for Points or Money that night. NO EXCEPTIONS.
6200 Pro Street 4x4 Truck Class
All General Truck Rules Apply 
1)
6200 lb. weight limit
2)
473 cubic inch limit (1% tolerance allowed)
3)
Vehicles limited to one (one-piece) carburetor.
4)
Factory Production Cast Iron OEM Heads – No Hemi Heads – No Aluminum Heads.  Head must have factory Casting numbers on them in factory location. No aftermarket cast iron heads allowed.
5)
Open exhaust okay, all exhaust must exit down and back.
6)
Must run stock frame and body.  Cutting out beds is allowed but must be covered. Bumpers must be ascetic to the body.
7)     Can have solid rear suspension. The rear axle must be solidly attached.
8)     No weights beyond factory front bumper
9)
Street legal DOT tires (REFER TO RULE 1 GENERAL TRUCK RULES) and no larger than 33” tall and 12.5” wide or 305R tire size. Front tires cannot track past center of rear tires, or vice versa. 
10) Must use OEM type transfer case
6200 Pro Stock 4x4 Truck Class
General Truck Rules Apply
1)
485 CID & 6200 LBS Class
2)
Street legal DOT tires (REFER TO RULE 1 GENERAL TRUCK RULES) and no larger than 33” tall and 12.5” wide or 305R tire size. Front tires cannot track the center of rear tires, or vice versa. No 17” Tires and Wheels.
3)
Can have solid rear suspension. Rear axle must be attached.
4)
Body must retain original location. No body lifts.
5)
Any single four-barrel manifold is allowed.
6)
Headers must go straight up and out of hood or down and back. They cannot turn down.
7)
If the bed is cut out, it must be covered.
8)
Any type of transfer case allowed.
9)
Hood is required. Holes in hood for headers only. Holes for breather must be 16 inches or with any hood scoop.
10)
Any heads are acceptable other than Hemi heads.
11)
All trucks have side shields from frame to bottom of head.
12)
Weight bar must not exceed 60 inches from center line of front axle. 
Diesel Trucks
2.6 Diesel 4x4 Truck Class
1) Maximum weight is 8000 lbs.
2) OEM Chassis is mandatory. The vehicle must retain the full OEM chassis. Wheel tubs, back half conversions, and tube chassis are prohibited. Must retain factory OEM wheelbase for make and model of body, not to exceed 158 inches.
3) The body must be an OEM truck body including the full bed floor. No flatbeds permitted. The body must retain the full sheet metal. After market hoods permitted. The hood must be closed and securely latched when hooked to the sled.
4) A complete engine must have a stock appearance except where otherwise noted in these rules. Maximum engine size will be 460 ci. The engine must be in an OEM location for the body to be used. The engine must have a 3/8” diameter cable surrounding the engine block. Cable is to be positioned between #1 and #2 cylinders and is to pass through manifolds. Cable will have 4-6 inches of slack. Two cable clamps at cable splice are required.
5) The cylinder head must be an OEM or OEM replica for brand of engine. Outside of cylinder head must measure factory width and length. No billet heads of any material. The head must retain factory OEM valve angle. No deck plates permitted.
6) Hook point to be no closer than 44” of centerline of rear axle. Maximum hitch height of 24” with a minimum of 3.75”x3” opening. A hitch must be stationary in all directions. The hitch must be framed mounted. The use of Reese style hitches is prohibited. Hitch must not exceed 25-degree angle from pivot point to hook point. No hitch supports or adjusters fastened to rear axle housing shall be above center point of rear axle. The pivot pin of drawbar can be no further forward than the centerline of rear axle.
7) Turbo is limited to 2.6” inducer bore. Bore must be smooth. No MAP Width Enhancement groove (MWE) allowed. The compressor wheel must protrude into 2.6” bore for 1/8”. Bore will be checked with a 2.605” turbo plug. Plug must not be able to enter inducer bore and contact wheel.
8) Turbo is limited to 2.6” inducer bore. Bore must be smooth. No MAP Width Enhancement groove (MWE) allowed. Compressor wheel must protrude into 1. 2.6” bore for 1/8”. Bore will be checked with a 2.605” turbo plug. Plug must not be able to enter bore.
9)  All vehicles must be equipped with upward pointing exhaust located either directly behind the cab or out of truck hood. Two 3/8” diameter bolts must be placed through the exhaust pipe in a cross pattern within one inch of each other and within 12 inches of turbo.
10)  Front hanging weights are allowed, not to exceed 60 inches forward from the centerline of front axle. Ballast may be added to the bed of truck but must be securely fastened.
11)  All trucks must have at least a six-inch-wide u-joint shield around the rear u-joint constructed of at least 5/16-inch steel or 3/8 aluminum that will safely contain the u-joint and the end of the driveshaft. All shields must be securely mounted to vehicles. Any front-shaft u-joints that can be visibly seen from side of truck must be shielded to contain the u-joint and the end of the driveshaft.
12) A fire extinguisher system is required. 2.5# fire extinguisher must be securely mounted within reach of driver. A complete OEM firewall is required.
13) All drivers must have a valid driver’s license and full SFI fire suit including helmet, neck brace, fire gloves, fire shoes or leather boots. Seatbelt/restrain must be worn.
14) Complete OEM floor pans are mandatory. Vehicles must maintain a complete firewall. Additional gauges and pillar pods are permitted.
15) Hand throttles permitted. Diesel fuel only. No propane or N02 or any other oxygen enhancers allowed.
16) Maximum of one P pump up to P7100 allowed. 13MM plunger limit. Ag governors permitted. The use of multiple high pressure common rail fuel pumps is legal.
17) OEM rear and front ends required, must have come factory in a one ton or smaller vehicle.
18) Axle shields are required. Shield to be .060” thickness steel or aluminum. A hole may be cut in one shield to allow operation of hub lock.
19) Safety switches (rain caps or guillotine) must shut off air to diesel engines. The switch will be securely mounted to the back of the vehicle. A 2 inch or bigger solid ring must be attached to the end of switch. Ring must be zip tied to the bracket switch. The switch must also be able to be activated in cab while driver is secured in vehicle.
20) Hydraulic steering permitted.
21) Suspension (Rear) - The upper mounting point for strut assembly must be in the factory location. Adjustable caster/camber pillow ball mounts are permitted. The lower control arm may be strengthened provided the factory mounting points are maintained. Strut tower braces, lower tie bars, sway bars, and limit straps are permitted. Traction bars and devices are permitted. Raising or lowering vehicle height with suspension modifications is permitted but must be bolted on only. Welds permitted for attachment to frame and axle only. Blocked suspension permitted. No air bags. Rear suspension may be made solid.
22) Must have a 3-way dump valve. Must be able to be pulled from the driver’s seat.
23) Tires must be DOT approved with maximum size of 35x12.50. No studded tires or tire chains. No alterations to the tires permitted. No bar or terra tires.
24) Dual wheels are prohibited.
25) OEM transmission and transfer case must be used, must have come factory in one ton or smaller vehicle.
26) Non-OEM transmissions are prohibited. Aftermarket torque converters, valve bodies, and internal components are permitted.
27) SFI bell housing and/or SFI blow proof bell housing or SFI blanket type shield must be used.
28) Water injections are prohibited.
29) Air to Air intercooler only. No cooling device is allowed for intercoolers. No ice boxes.
6200 Pro Stock 2 Wheel Drive Truck Class 
General truck Rules Apply
1)        Tire side is limited to 18.4 X 16.1 nothing bigger
2)
30 inches hitch height, no bigger
3)
540 cubic inch limit
4)
Weight limit 6200 lbs.
5)  Can run 2 carburetors. Must be naturally aspirated. Can run fuel injections.
6) Can run alcohol. If you run alcohol, you MUST wear full fire suit (Jacket, pants, mask, gloves, boots, and full-face helmet) Helmet must be DOT or Snell rated.
7) Trucks will be no longer than 15 ½ feet from center of rear axle to the most       forward position of the truck.  No weights further than 15 feet.
6200 DOT 2 Wheel Drive Truck Class  
General Truck rules Apply.
1) 525 Cubic Inch with 1% tolerance
2) 140” wheelbase, weights not to exceed 15 ft.
3) 15 ft center rear to farthest point
4) No aftermarket Transmissions. OEM transmissions & straight cut gears
5) Conventional Heads only (Aluminum or cast iron)
6) 14 inches from center of front of bell housing
7) Single carburetor, No sheet metal intakes
8) No planetary rear ends
9) DOT approved tires, no taller than 35 inches and no wider than 12/50. Wheels – 15/16 Max. 
10)   May adjust weights after you cross the scales.
11)  30-inch hitch height. 
12)  Can run alcohol.  If you run alcohol, you MUST wear full fire suit (Jacket, pants, mask, gloves, booths, and full-face helmet) Helmet must be DOT or Snell rated. 
13) Weight limit – 6200 lbs.
General Tractor Rules 
Full Fire suit (jacket, pants, leather shoes or racing shoes, helmet full face, Neck brace and harness are required.  Helmets must be DOT or SNELL rated.
1) The hitch point of drawbar cannot exceed twenty (20) inches above level ground.
2) The hitch point must be at least eighteen (18) inches back from center of rear axle.
3) All weights must be secured on tractors: any object falling free of the tractor during the pull is a disqualification, except for breakage. 
4) Wheelie bars must be able to support the weight of the tractor and be less than (10) inches above ground. 
5) Factory sheet metal must be in place to cover engine compartment,
6) All tractors must have a wide front end. 
7) All tractors must have front skid plates, excluding the 11,000 Hot Stock Class. Skid plate must be mounted in line with each frame rail and extend from the center of the front axle forward (on both sides) equal in strength to frame rail material.  Skid plate surface to be a minimum of 4 inches wide and 12 inches long with minimum 6-inch curve when measured from the from most part of the rolled edge.  Note: Skid plate must be able to support the weight of the front-end when checked with a jack.  Maximum ground clearance from bottom of front wheel rim not to exceed 4 inches with front tires in normal operating position. 
8) Must weigh 2 1/2lb. fire extinguisher and be mounted within arm’s reach of the driver.
9) Throttles must be of a dead man type setup or (double spring return to idle) One spring on hand throttle, and on the carburetor or injection pump. 

10) Tractors must be equipped with a working air shut off (diesel engines) or ignition kill(gas). A 2-inch ring must be attached to the ed and positioned 48 inches above ground and be no more than six inches off center and must be able to be pulled from the driver’s seat and be able to freely be pulled completely away from tractor per sled requirement. 
11) The exhaust pipe must have two (2) 3/8 bolts crossed to prevent turbo parts from flying out. 
12) PTO shafts must be covered or locked out. 
13) All tractors will be equipped with a SFI certified clutch blanket and turbo blanket.
14) Tractor rear ends and transmissions must be in stock appearing OEM, agriculture type, Using OEM adaptor plates. 
15) Tractors must be equipped with full side shields that cover the engine below crank shaft centerline, excluding the 11,000 Hot Stock Class. There must be a minimum of .060-inch-thick steel or aluminum.  They must be easily removed.
16) Inner shields made of ¼ inch aluminum of 1/8 steel is recommended.
17) Draw bar must be equipped with a steel hitching device not less than 1 ½ inch by 1 ½ inch square (1 1/2 round stock) and with a round hole minimum of 3 ¾ inch diameter.  The hook from the sled must freely fall into hitch. 
18) Tractors must be equipped with a functioning kill switch to disable the ignition system of a gasoline engine or an air shut off system on diesel engine. Kill switch must be in an easily accessible location. 
19) All tractors must be equipped with roll cages and 5-point harnesses excluding the 11,000 Hot Stock Tractor Class. 
6000 Pro Field Tractor Class
General Tractor Rules Apply
1) 6000 LB turbo and 6000 LB naturally aspirated tractors will pull in this class.
2) Any gasoline tractors may run on 4-barrel carburetor; will allow gas turbocharged motors with 361 cubic inches or less to run with no RPM limit.  Must use SFI approved clutch. 
3) Tractors will be equipped with a steel flywheel and pressure plate. Positively no gray cast metal allowed in any flywheel or clutch component.
4) Tractors will be equipped with a SFI SPEC 4.2 bell housing blanket.  Any exposed automatic type of transmission must be covered by a scatter shield. 
5) Sheet Metal needs to be in the family of the tractor.  Any AG motor with like brand AG rear end
6) Primary fuel shall be diesel or pump gas, no alcohol. No electronic controlled fuel injection allowed on gasoline or diesel engines.  No throttle base injection systems. 
7) No nitrous oxide or propane injection system allowed.
8) Diesel tractors are allowed to run a P Pump, and gasoline tractors are allowed to use one 4-barrel carburetor.
9) Diesel tractors may be converted to gasoline fuel systems. 
10)   Maximum tire size is 18.4 x 38. 
11)  Naturally aspirated, maximum of 650 cubic inch turbo tractors shall have a 360 cubic inch limit. 
12) Diesel tractors equipped with turbo or supercharger shall comply with the following additional rules:
3000 RPM limit Tractors shall have operative, factory equipped governors which will be checked by: visual retarding movement of the throttle linkage from governor cast to carburetor: and audible acceleration when clutch is engaged while holding brakes on with tractor in high gear.  Tractor shall be equipped with tack cable with one magnet (female connection from tractor) to hook to sled.  Verification and consequences for excessive RPM shall be the same as Hot Stock classes. Water & alcohol mix injections into intake allowed. 
        13)    All tractors will be equipped with individual workable rear wheel brakes.
                activated by the gearshift lever when the tractor is in reverse.
6500 Limited Super Stock Tractor Class
General Tractor Rules Apply
1) Tire Size is open. 
2) 650 Cubic Limit
3) Tractors will be equipped with a steel flywheel & pressure plate. Positively no gray cast metal allowed in any flywheel or clutch component. 
4) Tractors are equipped with a SFI SEC 4.2 Bell housing Blanket.  Any exposed automatic type of transmission must be covered by a scatter shield. 
5) Tractors with agriculture type engines; 360 cubic inches or less may run with (2) turbochargers. 
6) Tractors with agriculture type engine: 361 cubic inches or more may run with (2) turbochargers but must weigh 6000LBs.
9000 Pro-Field Tractor Class
General Tractor Rules Apply
1. Weight Class is 9000 LBS
2. Tires will be no wider than 25” or 38” maximum inside diameter.
3. RPM limits are as follows: 466 cu in and under are limited to 3500 RPM; over 466 cu in are limited to 3000 RPM.  50 rpm spikes allowed anything over is a one-time warning.  Secondly check if Rpms are over limit or cannot be read, puller is disqualified.
4. RPM checks will be done by two (2) Board Members with one checking the throttle while the other uses the tach.
5. Tractors will have a stock block with a cubic inch limit of 640.
6. Tractors may use “A” or “P” injection pump or stock appearing pump w/ 13mm pump limit.
7. Water injections are allowed.
8. Exhaust will have four (4) 3/8-inch bolts, two (2) ½ inch bolts or a turbo containment device within 2” of cast turbo housing at 90-degree angles.
9. The hitch will be 18 inches in length and 20 inches high.
10. Tractors may use a turbo of choice with a standard restriction of 3.00 inches maximum on the air inlet side of the turbo as close to the turbo as possible.  The restriction will be readily accessible for a tech check.
11. Only single-stage, exhaust-driven turbos will be allowed.  Turbochargers must be under the hood or completely shrouded with not less than .060 thick steel, except for the inlet exhaust pipes.
12. All tractors will be equipped with a five-point harness and have a roll cage to meet the requirements of the class.  (see General Rules section)
13. No intercoolers or ice boxes are allowed.
14. All tractors must run a steel flywheel.
15. Recast cylinder heads are allowed.  No Billet.  Cylinder head must retain OEM (Length/Width/Height) for engine application.  Valves must retain OEM angles for engine application.  2 valves per cylinder maximum.  The cylinder head must retain OEM bolt pattern for exhaust manifold and bolt pattern must be used to attach the exhaust manifold and intake.  The manifold must bolt 90 degrees to head.  No overhead cams permitted. 
16. The engine must run on factory designed fuel.
17. 2 springs to pull throttle back to idle: 1 on pump 1 on throttle handle.
18. 11,000 hot stock tractors will be allowed to hook in the 9000 pro-field class under one of the following options:
a. Weigh 9000 lbs. and run under the 9000 Pro-Field rules if, and only if they meet ALL the rules and safety requirements of the 9000 Pro-Field class. (This includes roll cages, steel flywheels, side shields, etc.)
b. Weigh 11,000 lbs. and run under the 11,000 Hot Stock rules.
c. You can only pull in one class.
11000 Hot Stock Tractor Class
General Tractor Rules Apply
1)
466 Cubic inch limit: any motor over 466 Cubic inches must have factory stroke and bore for that brand of tractor, up to a maximum of 585 cubic inches
2)
Tractor is limited to a single turbo charger. You can run a 3LM up to S300 2.36 inlet.  The S300 is limited to 90 housing with part #177272 or 100 housing with part #177209.  Must be out of the box with no modifications.  The 360-degree thrust can be installed. 
3)
Injection pump can be up to a (P7100) 13MM barrel and plunger pump max. 
4)
Max. RPMS 2950
5)         Must have working tack cable with 1 magnet (female connections from the    tractor) to hook to the sled.  CANNOT tack more than 2950 RPMS per tack box during the pull.  If the tack box records a greater than 2950 during the pull, that tractor will be disqualified, unless the tack box is inaccurate.  An alternative method of checking RPMS will be a hand-held tack at the end of the track.  Flag officials at the end of the track will be responsible for reading the tack box and determining which tractors to hand check RPMs.  The consequences for exceeding the RPM limit is as follows: 
1) First offense:   forfeit prize money and all points for that event.
2) Second offense: forfeit prize money and all points for that event.
3) Third offense: 1 year and 1 day suspension for that tractor for all classes in which it competes. 
The first and second offenses in one weight class do not add to violations in another limited RPM class. 

6)  Tractors must have a minimum factory ROPS roll bar and seat belt.  If running with anything other than a three-bar roll cage, tractor MUST have fenders able to support the weight of the driver.  Three bar roll cages and a five-point harness are recommended. 
7)  Top cut tires. No alterations of any kind to the facing of the lung.  Max Tire size 20.8 x 38.
8) Water injections will be allowed.  No alcohol, propane or nitrous injection allowed. 
9) Only OEM inter coolers can be used but must run through the motor. 
10) All tractors will be equipped with a clutch blanket or a minimum 5 inch wide by ½ inch thick steel band around the bell housing. 
11)   Front axle skid plate and engine side shields are recommended but are not required.  Must have a factory OEM wide front end. 
12)   Tube frames are permitted.
13)   Tie bars are mandatory.
9500 Limited Open Tractor Class 
Non-Sanctioned Class 
1)  640 Cubic Inch plus 1%
2) OEM heard or recast for the make & model with all head bolts in stock location.
3) No overhead cams are allowed.
4) Must comply with all General Tractor Rules & have all safety equipment.
5) Diesel Fuel only & water injection allowed.
6) 25’ x 38” maximum tire size
7) No component chassis allowed.
8) 16 MM maximum on injection pumps P7100 or sigma allowed.
11000 Farm Stock Tractor Class
General Tractor Rules Apply
1)
Tractor engines can run up to 3000 governed high idle.
2)
Tractors must be equipped with factory intake manifold and carburetor. (The same as the parts book would show.)
3)
Tractor must have factory equipped governor and to be operative. To be checked by (A) visual retarding movement of throttle linkage from governor case to carburetor and (B) audible acceleration when clutch is engaged while holding brakes on with tractor in high gear.
4)
All weights must be in a factory weight rack or bolted to wheels.  Front weights and brackets must be in stock location and bolted to rear wheels.
5)
Tractors must be stock pump, bore and stoke for make and model.
6) Tires must have manufacture size and markings.
10500 Hot Farm Tractor Class 

1) Weight will be 10500. Maximum tire size 20.8 (uncut) or 18.4 (double cut)

2) Turbo and non turbo tractors will run in the same class. Turbo tractors will have standard restrictions of 2.8 in on air inlet side of turbo. 

3) 3000 RPM limit, you must have a sensor on your tractor, or you will not be allowed to pull. 

4) Gasoline powered tractors can have any agriculture updraft carburetor. No alcohol tractors. 

5) May run A pump, max. No pump or sigma pumps are allowed.

6) Tractors will have operative factories equipped with governors. Must have dead man throttle.  

7) Tractor must have a 2/12 lb. fire extinguisher mounted within the reach of the driver. 

8) Tractors will have a backup light, minimum of 2 inches in diameter activated by gearshift lever when tractor is placed in reverse. 

9) Tractors must have roll bar and 4-point harness. 

10) No water injection is allowed. 

11) Drivers must wear full-faced helmet, gloves, neck braces, fire pants, fire coat and racing shoes or leather boots. 

Sleds
1)         All sleds must be of a mechanical device with rider on sled when it is in operation. All sleds also must have workable brakes with a red light that comes on when the brake is applied.
2)
All sleds must be a rigid design and stay on the ground to prevent excessive bouncing.
3)
All weight transfer mechanisms and sleds as a unit must have passed a safety inspection by the competition committee.
4)         The sled hitch must be a centered single design with a pivot design not to exceed 30 degrees nor less than 10 degrees.
5)
The length of the hitch on an official sled shall be 36 inches for mini’s, 46 inches for truck (plus or minus ½ inch) measured from the point of the hitch rearward to the point the chain attaches to the sled. The sled point of hitch shall not be more than four inches above ground level.
To Sell the sled
It will take 2/3 of all membership votes to sell the sled out from the association.  The Executive Board has the final say.
                                                                 Notes
________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________
